• Bandwidth: 1.3 MHz (G = 1)

• Low noise: 8 nV/√Hz, 0.2 μVpp

• Voltage range : 2 V and – 2V